Field      | Description
---------- | -----------
H_20mmh    | Combined hazard class for a peak 15-minute rainfall intensity of 20 mm/hour
H_20mmh_LG | Legend entry of combined hazard class for a peak 15-minute rainfall intensity of 20 mm/hour
P_20mmh    | Debris-flow likelihood for a peak 15-minute rainfall intensity of 20 mm/hour
P_20mmh_LG | Legend entry of debris-flow likelihood for a peak 15-minute rainfall intensity of 20 mm/hour
V_20mmh    | Potential sediment volume (meters^3) for a peak 15-minute rainfall intensity of 20 mm/hour
V_20mmh_LG | Legend entry of potential sediment volume (meters^3) for a peak 15-minute rainfall intensity of 20 mm/hour
Vmin_20mmh | Lower bound of the 95% confidence interval of volume estimates for a peak 15-minute rainfall intensity of 20 mm/hour
Vmax_20mmh | Upper bound of the 95% confidence interval of volume estimates for a peak 15-minute rainfall intensity of 20 mm/hour
H_24mmh    | Combined hazard class for a peak 15-minute rainfall intensity of 24 mm/hour
H_24mmh_LG | Legend entry of combined hazard class for a peak 15-minute rainfall intensity of 24 mm/hour
P_24mmh    | Debris-flow likelihood for a peak 15-minute rainfall intensity of 24 mm/hour
P_24mmh_LG | Legend entry of debris-flow likelihood for a peak 15-minute rainfall intensity of 24 mm/hour
V_24mmh    | Potential sediment volume (meters^3) for a peak 15-minute rainfall intensity of 24 mm/hour
V_24mmh_LG | Legend entry of potential sediment volume (meters^3) for a peak 15-minute rainfall intensity of 24 mm/hour
Vmin_24mmh | Lower bound of the 95% confidence interval of volume estimates for a peak 15-minute rainfall intensity of 24 mm/hour
Vmax_24mmh | Upper bound of the 95% confidence interval of volume estimates for a peak 15-minute rainfall intensity of 24 mm/hour
H_28mmh    | Combined hazard class for a peak 15-minute rainfall intensity of 28 mm/hour
H_28mmh_LG | Legend entry of combined hazard class for a peak 15-minute rainfall intensity of 28 mm/hour
P_28mmh    | Debris-flow likelihood for a peak 15-minute rainfall intensity of 28 mm/hour
P_28mmh_LG | Legend entry of debris-flow likelihood for a peak 15-minute rainfall intensity of 28 mm/hour
V_28mmh    | Potential sediment volume (meters^3) for a peak 15-minute rainfall intensity of 28 mm/hour
V_28mmh_LG | Legend entry of potential sediment volume (meters^3) for a peak 15-minute rainfall intensity of 28 mm/hour
Vmin_28mmh | Lower bound of the 95% confidence interval of volume estimates for a peak 15-minute rainfall intensity of 28 mm/hour
Vmax_28mmh | Upper bound of the 95% confidence interval of volume estimates for a peak 15-minute rainfall intensity of 28 mm/hour
H_32mmh    | Combined hazard class for a peak 15-minute rainfall intensity of 32 mm/hour
H_32mmh_LG | Legend entry of combined hazard class for a peak 15-minute rainfall intensity of 32 mm/hour
P_32mmh    | Debris-flow likelihood for a peak 15-minute rainfall intensity of 32 mm/hour
P_32mmh_LG | Legend entry of debris-flow likelihood for a peak 15-minute rainfall intensity of 32 mm/hour
V_32mmh    | Potential sediment volume (meters^3) for a peak 15-minute rainfall intensity of 32 mm/hour
V_32mmh_LG | Legend entry of potential sediment volume (meters^3) for a peak 15-minute rainfall intensity of 32 mm/hour
Vmin_32mmh | Lower bound of the 95% confidence interval of volume estimates for a peak 15-minute rainfall intensity of 32 mm/hour
Vmax_32mmh | Upper bound of the 95% confidence interval of volume estimates for a peak 15-minute rainfall intensity of 32 mm/hour
H_36mmh    | Combined hazard class for a peak 15-minute rainfall intensity of 36 mm/hour
H_36mmh_LG | Legend entry of combined hazard class for a peak 15-minute rainfall intensity of 36 mm/hour
P_36mmh    | Debris-flow likelihood for a peak 15-minute rainfall intensity of 36 mm/hour
P_36mmh_LG | Legend entry of debris-flow likelihood for a peak 15-minute rainfall intensity of 36 mm/hour
V_36mmh    | Potential sediment volume (meters^3) for a peak 15-minute rainfall intensity of 36 mm/hour
V_36mmh_LG | Legend entry of potential sediment volume (meters^3) for a peak 15-minute rainfall intensity of 36 mm/hour
Vmin_36mmh | Lower bound of the 95% confidence interval of volume estimates for a peak 15-minute rainfall intensity of 36 mm/hour
Vmax_36mmh | Upper bound of the 95% confidence interval of volume estimates for a peak 15-minute rainfall intensity of 36 mm/hour
H_40mmh    | Combined hazard class for a peak 15-minute rainfall intensity of 40 mm/hour
H_40mmh_LG | Legend entry of combined hazard class for a peak 15-minute rainfall intensity of 40 mm/hour
P_40mmh    | Debris-flow likelihood for a peak 15-minute rainfall intensity of 40 mm/hour
P_40mmh_LG | Legend entry of debris-flow likelihood for a peak 15-minute rainfall intensity of 40 mm/hour
V_40mmh    | Potential sediment volume (meters^3) for a peak 15-minute rainfall intensity of 40 mm/hour
V_40mmh_LG | Legend entry of potential sediment volume (meters^3) for a peak 15-minute rainfall intensity of 40 mm/hour
Vmin_40mmh | Lower bound of the 95% confidence interval of volume estimates for a peak 15-minute rainfall intensity of 40 mm/hour
Vmax_40mmh | Upper bound of the 95% confidence interval of volume estimates for a peak 15-minute rainfall intensity of 40 mm/hour
H_50mmh    | Combined hazard class for a peak 15-minute rainfall intensity of 50 mm/hour
H_50mmh_LG | Legend entry of combined hazard class for a peak 15-minute rainfall intensity of 50 mm/hour
P_50mmh    | Debris-flow likelihood for a peak 15-minute rainfall intensity of 50 mm/hour
P_50mmh_LG | Legend entry of debris-flow likelihood for a peak 15-minute rainfall intensity of 50 mm/hour
V_50mmh    | Potential sediment volume (meters^3) for a peak 15-minute rainfall intensity of 50 mm/hour
V_50mmh_LG | Legend entry of potential sediment volume (meters^3) for a peak 15-minute rainfall intensity of 50 mm/hour
Vmin_50mmh | Lower bound of the 95% confidence interval of volume estimates for a peak 15-minute rainfall intensity of 50 mm/hour
Vmax_50mmh | Upper bound of the 95% confidence interval of volume estimates for a peak 15-minute rainfall intensity of 50 mm/hour
H_60mmh    | Combined hazard class for a peak 15-minute rainfall intensity of 60 mm/hour
H_60mmh_LG | Legend entry of combined hazard class for a peak 15-minute rainfall intensity of 60 mm/hour
P_60mmh    | Debris-flow likelihood for a peak 15-minute rainfall intensity of 60 mm/hour
P_60mmh_LG | Legend entry of debris-flow likelihood for a peak 15-minute rainfall intensity of 60 mm/hour
V_60mmh    | Potential sediment volume (meters^3) for a peak 15-minute rainfall intensity of 60 mm/hour
V_60mmh_LG | Legend entry of potential sediment volume (meters^3) for a peak 15-minute rainfall intensity of 60 mm/hour
Vmin_60mmh | Lower bound of the 95% confidence interval of volume estimates for a peak 15-minute rainfall intensity of 60 mm/hour
Vmax_60mmh | Upper bound of the 95% confidence interval of volume estimates for a peak 15-minute rainfall intensity of 60 mm/hour
I15_50_LG  | Legend entry of peak 15-minute rainfall accumulation (in mm) needed for a debris-flow probability of 50%
I15_50     | Peak 15-minute rainfall intensity (in mm/hour) needed for a debris-flow probability of 50%
R15_50     | 15-minute rainfall accumulation (in mm) needed for a debris-flow probability of 50%
I15_75     | Peak 15-minute rainfall intensity (in mm/hour) needed for a debris-flow probability of 75%
R15_75     | 15-minute rainfall accumulation (in mm) needed for a debris-flow probability of 75%
I30_50     | Peak 30-minute rainfall intensity (in mm/hour) needed for a debris-flow probability of 50%
R30_50     | 30-minute rainfall accumulation (in mm) needed for a debris-flow probability of 50%
I30_75     | Peak 30-minute rainfall intensity (in mm/hour) needed for a debris-flow probability of 75%
R30_75     | 30-minute rainfall accumulation (in mm) needed for a debris-flow probability of 75%
I60_50     | Peak 60-minute rainfall intensity (in mm/hour) needed for a debris-flow probability of 50%
R60_50     | 60-minute rainfall accumulation (in mm) needed for a debris-flow probability of 50%
I60_75     | Peak 60-minute rainfall intensity (in mm/hour) needed for a debris-flow probability of 75%
R60_75     | 60-minute rainfall accumulation (in mm) needed for a debris-flow probability of 75%
T          | ('Terrain variable for the M1 likelihood model. Proportion of catchment area that is both (1) burned at moderate or high severity, and (2) has a slope >= 23 degrees',)
F          | Fire variable for the M1 likelihood model. Mean catchment dNBR / 1000
S          | Soil variable for the M1 likelihood model. Mean catchment KF-factor
Bmh_km2    | Catchment area burned at moderate or high severity in kilometers^2. Used to estimate potential sediment volumes.
Relief     | Watershed relief in meters. Used to estimate potential sediment volumes.
Area_km2   | Total catchment area in kilometers^2
BurnRatio  | Proportion of catchment area that is burned
ConfAngle  | Confinement angle in degrees
DevArea    | Developed catchment area in kilometers^2
Slope      | Slope gradient (rise / run) along each stream segment
InPerim    | Whether each stream segment intersects the fire perimeter
